**Basic variant with inner seal**

for buildings with a basement

Article Code: MSH PolySafe GV2

Article number: 1560000002

GTIN: 4052487162692

Brand: Hauff-Technik

For the collective feeding in and sealing of all supply lines (power/water/telecommunications/gas). The MSH PolySafe GV2 is a basic module supplemented with the following separately available section sealing elements, modules or the MSH PolySafe wall sleeve: MSH PolySafe sealing element set (section sealing elements) Module 3: Insulation plate for insertion in existing perimeter insulation Module 6: External sealing element with 90 mm sealing width for double/element walls without additional damp-proofing Module 6.2: External sealing element with outer flange for integration in existing building damp-proofing in double/element walls Additional supplements are possible.

Dimensions: Sealing width: 60 mm; Compatible with core drill/wall sleeve: ID: 199 - 203 mm; Maximum wall thickness: 500 mm (special lengths on request)

Material: Inner seal: Fibre-glass reinforced polyamide/EPDM; Sleeve pipes: PVC; Screws: stainless steel V2A (AISI 304L)

Application range: Water exposure class DIN 18533: W1-E and W2.1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight to 1.0 bar; radon-proof

Tests/Standards: DVGW VP 601

Features: testable reliability in double/element walls due to built-in leakage test facility; reliable installation due to front panel with integrated spirit level; visual installation reliability due to built-in inspection opening

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de