**Basic variant with inner seal**

Material: Front plate: glass fibre reinforced polyamide; Rubber: EPDM; Sleeve pipe: PVC-U; Screws: stainless steel V2A (AISI 304L)

Application range: Water exposure class DIN 18533: W1-E and W2.1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight to 1.0 bar; radon tight

Tests/Standards: DVGW VP 601

Features: optical and tangible installation security due to integrated control opening

Article Code: ESH PolySafe GV1

Article number: 1910000000

GTIN: 4052487162821

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de