**Basic variant with inner seal**

for buildings with a basement

Article Code: ESH PolySafe GV1

Article number: 1910000000

GTIN: 4052487162821

Brand: Hauff-Technik

Gastight and watertight building entry for buildings with a basement for gas, water, power or telecommunications services. Basic variant 1 (GV 1) with inner seal 40 mm sealing width. As this is a modular system, the outer seal can be freely selected as appropriate for the type of wall. Compatible with core drills or wall sleeves ∅: 100 mm (e.g. FZR 100/x). Gas valve/closed sealing element and external module are not included in the scope of delivery (see accessories).

Dimensions: Sealing width: 40 mm; Core drill/wall sleeve: ID 99 - 103 mm; Sleeve pipe OD: 75 mm, 600 mm long; Maximum wall thickness: 500 mm (special lengths on request)

Material: Front plate: glass fibre reinforced polyamide; Rubber: EPDM; Sleeve pipe: PVC-U; Screws: stainless steel V2A (AISI 304L)

: Water exposure class DIN 18533: W1-E and W2.1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight to 1.0 bar; radon-proof

Tests/Standards: DVGW VP 601

Features: Visual and physical installation control thanks to integrated inspection opening

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de