**Polymer flange**

for retrofit installation

Article Code: HSI90 DFK

Article number: 3030466887

GTIN: 4052487240529

Brand: Hauff-Technik

Plastic flange for retrofit dowelling using core drills or for screwing onto housing. Used for the gastight and watertight connection of system seals for cables and cable ducts.

Dimensions: Length x width: 185 x 185 mm; Recommended centre distance for core drills: 200 mm; Core drills max. Ø: 100 mm; Build-up in front of the wall including surface seal: 40 mm

Material: Flange: glass fibre reinforced polyamide; Surface seal: EPDM; Fastenings: stainless steel V4A (AISI 316L)

Application range: Water exposure class DIN 18533: W1-E and W2.1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight to 2.0 bar

Features: with integrated spirit level; Tested solution for use in pre-applied membrane sheet systems

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de