**Membrane injection system**

for buildings without a basement

Article Code: 2LINE MIS25 1x6-13 PRO

Article number: 3030477964

GTIN: 4052487242905

Brand: Hauff-Technik

For reliable sealing of fibre optic cables. For installation in all standard wall types to DIN 18533 W1.1-E, W1.2-E, W2.1-E and waterproof concrete according to DIN 1045. Includes 2-component resin RESINATOR.

Dimensions: for drill holes Øi: 25 mm; for wall thicknesses starting from 150 mm

Material: Membrane sleeve: TPE; Foil flange: Aluminium-plastic composite foil with butyl rubber; Wall terminator element: PCFR

: Water exposure class DIN 18533: W1-E and W2.1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight to 1.0 bar

Number of cables/medium: 1

suitable for medium pipe OD (mm): 6-13

Features: controlled RESINATOR resin discharge thanks to proven membrane injection system; tool-free assembly with RESINATOR double syringe; Horizontal or angled installation up to 45° angle

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de