**Basic insert - round design**

for buildings without a basement

For the collective feeding in and sealing of all supply lines (power, water, telecommunications, gas). Round design.

Material: Wall sleeve: ABS; Installation fixture: St37

Load case: Waterproof concrete stress class 2; Waterproof concrete stress class 1

Tightness: gastight and watertight to 1.0 bar

Tests/Standards: DVGW VP 601

Lines side by side: 4

Features: Variable height adaptation to the finished floor level

Article Code: MSH Basic FUBO EBTM

Article number: 1550100048

GTIN: 4052487030366

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de