**Multi-line basic insert, arranged side by side**

For buildings without a basement

For the collective feeding in and sealing of supply lines (power, water, telecommunications, gas). The four supply lines are arranged side by side.

Dimensions: Width: 216 mm; Length: 579 mm; Height: 270 mm

Material: Wall sleeve frame parts: ABS; Installation fixture: St37

Load case: Waterproof concrete stress class 1; Waterproof concrete stress class 2; DIN 18533 W1.1-E; DIN 18533 W1.2-E

Tightness: gastight and watertight to 1.0 bar

Tests/Standards: DVGW VP 601

Item: Mehrsparten-Rohbauteil Reihenanordnung

Features: Variable height adaptation to the finished floor level; easy integration of the vapour barrier using the adhesive ribbon

Article Code: MSH Basic FUBO SR4 EBT

Article number: 1551008600

GTIN: 4052487204804

Brand: Hauff-Technik

**Technical drawings**

[Maße MSH Basic FUBO SR4 (.PDF)](https://db.hauff-technik.de/files/912/3/BEMA_UNG_FUBO_SR4.PDF)

Ctrl + click on the link to open in your browser

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de