**Compound injection unit**

for wet installation of MSH PolySafe MV (grouting)

For wet installation of multi-line building entry system (grouting) in conjunction with Hauff-Beto-Fix void-filling mortar. Compound surface of the MSH PolySafe VVR 45° is a 2-level installation.

Material: Filler plate: stainless steel 1.4301 (AISI 316L); Clamping fixture: galvanised steel; Surface seal: NBR

Features: 4 holding pins for self-centring

Article Code: MSH PolySafe VFV45

Article number: 1591000121

GTIN: 4052487038942

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de