**Wall entry pipe bend 160**

for district heating lines

For the feeding in and sealing of district heating supply lines through the floor slab. Positioning with separately available clip system on the district heating installation fixture and combination with spiral hose system and sealing elements.

Dimensions: Pipe bend radius: max. 1,000 mm

Material: PVC

Load case: Waterproof concrete stress class 1; Waterproof concrete stress class 2; DIN 18533 W1.1-E; DIN 18533 W1.2-E

Article Code: MSH Basic FUBO-FIX RB160 r1000

Article number: 1900500160

GTIN: 4052487157438

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de