**Single-line building entry ZAPPO**

for buildings with a basement

Building entry installed from the inside of the building for trenchless building connection. Can be used for uncontrolled drilling rockets in conjunction with driving pipes OD 75 mm.

Dimensions: Core drill: ID: 99 - 103 mm; Driving pipe: OD 75 mm

Material: Front panel and twist protection flaps: Fibre glass reinforced polyamide; Rubber: EPDM; Rear press ring and outer sealing element: stainless steel V2A (AISI 304L); Centring ring: stainless steel V2A (AISI 304L); Screws: stainless steel V2A (AISI 304L); Screws: stainless steel V2A (AISI 304L)

Load case: Waterproof concrete stress class 1; Waterproof concrete stress class 2; DIN 18533 W1.1-E; DIN 18533 W1.2-E

Tightness: gastight and watertight to 1.0 bar

Tests/Standards: DVGW VP 601

Features: No groundwork at the property; Continuous gastight empty conduit system

Article Code: ESH PolySafe VT75

Article number: 1910010000

GTIN: 4052487165303

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de