**Combined building entry for gas**

for buildings with a basement

Combined building entry for gas with gas valve manufactured by Schuck, DN 100, for use in core drills or wall sleeves ID 200 mm.

Dimensions: Core drill/wall sleeve ID: 200 mm; Wall thickness: 240 - 800 mm

Material: Seal insert: stainless steel V2A (AISI 304L); Rubber: EPDM

Load case: Waterproof concrete stress class 2; Waterproof concrete stress class 1

Tightness: gastight and watertight to 1.0 bar

Item: Gebäudeeinführung Gas für unterkellerte Gebäude

Article Code: HSB SKIBFGT-PESS-PE100-TE DN100 BL1540

Article number: 1990800020

GTIN: 4052487054447

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de