**Basic insert**

for buildings without a basement

Basic insert and installation fixture for setting in concrete in the floor slabs of buildings without a basement. For the compact entry of gas or water services, DN 80. The combined building entry HEK and the flexible spiral hose are not included in the scope of delivery.

Dimensions: Basic insert: ID 150 mm

Material: Basic insert: PVC-U; Sleeve: EPDM; Water barrier flange: EPDM; Installation fixture: St37

Load case: Waterproof concrete stress class 1; Waterproof concrete stress class 2; DIN 18533 W1.1-E; DIN 18533 W1.2-E

Tightness: gastight and watertight to 1.0 bar

Item: Rohbauteil

Features: Variable height adaptation to the finished floor level

Article Code: ESG150 FUBO EBTMA

Article number: 1990801010

GTIN: 4052487054584

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de