**Polymer flange**

for retrofit dowelling

Plastic flange for retrofit dowelling using core drills or for screwing onto housing. Used for the gastight and watertight connection of system seals for cables and cable ducts.

Dimensions: Length x width: 235 x 235 mm; Recommended centre distance for core drills: 250 mm; Core drills max. Ø: 150 mm; Structure in front of wall including surface seal: 63 mm

Material: Flange: glass fibre reinforced polyamide; Surface seal: EPDM; Fastenings: stainless steel V4A (AISI 316L)

Load case: Waterproof concrete stress class 1; Waterproof concrete stress class 2; DIN 18533 W1.1-E; DIN 18533 W1.2-E; DIN 18533 W2.1-E

Tightness: gastight and watertight to 2.5 bar

Features: With integrated spirit level; Tried and tested solution for use in fresh concrete composite systems

Article Code: HSI150 DFK

Article number: 2118010020

GTIN: 4052487156264

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de