**Cement-coated wall sleeve with sleeve**

floor entry for Hateflex spiral hose

Cement-coated wall sleeve with sleeve Cable entry system in the form of a floor slab entry system with break-resistant, inherently stable cement-coated wall sleeve for the connection of the Hateflex 14150 spiral hose with the sleeve method.

Dimensions: Wall sleeve ID: 150 mm; Length (not including sleeve): 500 mm

Material: Pipe: PVC-U; Closing cover: PE; Sleeve: EPDM; Clamping straps: W4

Load case: Waterproof concrete stress class 2; Waterproof concrete stress class 1

Tightness: gastight and watertight

Item: Zement-Verbund-Rohr mit Manschette

Features: Special coating creates a homogeneous bond with the concrete; The cement-coated wall sleeve can be cut to size straight or at an angle once the floor has been finished

Article Code: KES MA150 ZVR150/500

Article number: 2125502000

GTIN: 4052487139991

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de