**Aluminium flange**

for retrofit dowelling

For retrofit dowelling with core drills or for screwing onto housings. Used for the gastight and watertight connection of system covers for cables and cable ducts.

Dimensions: Length x width: 185 x 185 mm; Recommended centre distance for core drills: 200 mm; Core drills maximum Ø: 90 mm; Structure in front of wall including surface seal: 46 mm

Material: Flange: aluminium with cathodic coating; Surface seal: chloroprene (CR); Fastenings: stainless steel V4A (AISI 316L)

Load case: Waterproof concrete stress class 1; Waterproof concrete stress class 2; DIN 18533 W1.1-E; DIN 18533 W1.2-E; DIN 18533 W2.1-E

Tightness: gastight and watertight to 2.0 bar

Features: Cathodic coating for optimum corrosion protection

Article Code: HSI90 DF

Article number: 2203010001

GTIN: 4052487060646

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de