**Fixed/loose flange wall sleeve made from stainless steel**

for retrofit dowelling for black tank according to DIN 18533

For dowelling with wall sleeves, core drills or breakthroughs.

Dimensions: Standard fixed flange Øa equal to the relevant wall sleeve Øi + approx. 330 mm (for one passage); Standard upper length: 80 mm

Material: Fixed/loose flange wall sleeve: stainless steel V2A (AISI 304L) or V4A (AISI 316L); Fastenings: stainless steel V4A (AISI 316L); Closing cover: PE

Load case: DIN 18533 W2.1-E; DIN 18533 W2.2-E

Tightness: gastight and watertight

Wall sleeve ID (mm) D1: 300

Fixed flange OD (mm) D2: 630

Loose flange OD (mm) D3: 620

Wall sleeve wall thickness (mm) S: 2

Article Code: FLFA1x300/80/0 DIN18533 A2

Article number: 2500400007

GTIN: 4052487062381

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de