**Membrane injection system**

for buildings with a basement

Building entry installed from the inside of the building for trenchless building connection. Can also be used for uncontrolled drilling rockets in conjunction with driving pipes OD 63 mm.

Dimensions: For core drills: ID 99 - 103 mm; For wall thicknesses: from 240 to 600 mm

Material: Front plate: glass fibre reinforced polyamide; Sealing rubber, flange, seal insert and counter-bearing: EPDM; Pipe: PVC-U; Screws and washers: stainless steel V2A (AISI 304L)

Load case: Waterproof concrete stress class 1; Waterproof concrete stress class 2; DIN 18533 W1.1-E; DIN 18533 W1.2-E

Tightness: gastight and watertight to 1.0 bar

wall thickness (mm): 240 - 600

Features: No groundwork at the property; Universal building entry with membrane injection system for drill holes in the most common types of wall; Controlled ejection of resin through slit membrane hose

Article Code: MIS100ND VT63

Article number: 2900300800

GTIN: 4052487174299

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de