**Single building entry MIS**

with membrane injection system

Dimensions: For core drills Ø: 99 - 103 mm; For wall thicknesses: from 240 to 600 mm

Material: Flange component, wall rosette, membrane hose: EPDM; Resin filler hose: PE; Fast arrangement fixture: glass fibre reinforced polyamide/ABS; Sealing tape: butyl

Load case: Waterproof concrete stress class 1; Waterproof concrete stress class 2; DIN 18533 W1.1-E; DIN 18533 W1.2-E; DIN 18533 W2.1-E

Tightness: gastight and watertight to 1.0 bar

Tests/Standards: DVGW VP 601

Number of cables/medium overall: 1

Number of cables/medium: 1

​Suitable for medium pipe OD (mm): 58 - 64

wall thickness (mm): 240 - 600

Packing unit: 6

Features: Universal building entry with membrane injection system for drill holes in the most common types of wall; Controlled ejection of resin through slit membrane hose

Article Code: MIS100D 1x58-64 Gas

Article number: 3030300100

GTIN: 4052487220224

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de