**Above-ground building entry**

for glass fibre empty conduits of 7 - 12 mm

Features: Universal building entry for drill holes in the most common types of wall. Enables horizontal or angled installation up to a 45° angle. Low-impact sealing of fibre optic cables by means of sealant.

Material: Wall terminator element: Flame-retardant polycarbonate; Screws: stainless steel V2A (AISI 304L)

​Suitable for medium pipe OD (mm): 7-12

Article Code: 2LINE OHE 1x7-12 SET10

Article number: 3030340562

GTIN: 4052487240512

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de