**Polymer flange**

for retrofit dowelling

Plastic flange for retrofit dowelling using core drills or for screwing onto housing. Used for the gastight and watertight connection of system seals for cables and cable ducts.

Dimensions: Length x width: 185 x 185 mm; Recommended centre distance for core drills: 200 mm; Core drills max. Ø: 100 mm; Structure in front of wall including surface seal: 40 mm

Material: Flange: glass fibre reinforced polyamide; Surface seal: EPDM; Fastenings: stainless steel V4A (AISI 316L)

: ; ; ; ;

Tightness: gastight and watertight to 2.0 bar

: With integrated spirit level; Tried and tested solution for use in fresh concrete composite systems

: HSI90 DFK

: 3030466887

GTIN: 4052487240529

**Hauff-Technik GmbH & Co. KG**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de