**Multi-line building package**

for buildings with a basement

For the collective feeding in and sealing of all supply lines (power, water, telecommunications, gas). Comprising: MSH PolySafe basic variant 1 and external sealing element MSH PolySafe M6.2 with universal sealing elements: electric: SDE 1x26-29/36-39/43-46/48-51, drinking water: SDW 1x32/40/50, communications: SDK 1x13-21+3x7-13+1x5-13, gas assembly kit Schuck+RMA incl. blind sealing MBHP DN25 D0 MSH fixtures Set4, comprising: 4 x sleeve caps (2 x MS78U 1x24-52, 1 x MS78K 1x13-21+3x7-13+1x5-12, 1 x MS78 D0) 16-piece Pipe connection set RAS16, universal gas tubing plug ABG63/70/78 1x32/40/50 Universal insulation disk MSH PolySafeM3 (Module 3) Ø199/320mm Tube of lubricant GMT

Dimensions: Compatible with core drill/wall sleeve: ID: 199 - 203 mm; Maximum wall thickness: 500 mm (special lengths on request)

Application range: Water exposure class DIN 18533: W1-E and W2.1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight to 1.0 bar; radon tight

Tests/Standards: DVGW VP 601

Features: Integrated leak test equipment; Reliable installation due to front panel with integrated spirit level; optical and tangible installation security due to integrated control opening

Article Code: MSH PolySafe BHP

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de