**BD-Fix**

Slab entry

For connecting KG/HT pipes. Gas and watertight connection to the base plate thanks to integrated lip seal.

Dimensions: Pipe lenght: 500 mm

Material: KG pipe: PVC-U/KG2000 pipe: PP; Lip seal: TPE

Application range: Waterproof concrete stress class 1 and 2

Tightness: pressure-tight up to 5,0 bar - corresponds to 50 m water column

Features: ready for installation in the slab

Article Code: BDF

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de