**Connection wall sleeve**

for installation in double walls/element walls

Wall pipe for installation in double walls/element walls. With three 3-ribbed seals as a water barrier in each layer of concrete. For the direct connection of a smooth duct DN 110 with plug-in/glue-in socket.

Material: Rubber sleeve and 3-ribbed seals: EPDM; Sleeve cover: ABS; Clamping strap: Steel St sn (W1); Closing cover: PE; Pipe: PVC-U

Application range: Water exposure class DIN 18533: W1-E and W2.1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight; radon tight

Features: Integrated flange connection

Article Code: AFRE 100/X

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de