**Bellmouth Wall Sleeve**

for setting in concrete

For installation flush with the formwork. Integrated Bellmouth shape on one side. Middle flange serves as water barrier.

Material: ABS

Tightness: gastight and watertight to 1.0 bar, right after concreting

Features: Frame connection system for creation of packages on site – compatible with all three sizes; Easy adjustment to the wall thickness on site – using available cable ducts

Article Code: BWS

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de