**Individual press seal**

Material: Press plates, screws, nuts and washers: rust-free stainless steel V2A (AISI 304L) or V4A (AISI 316L); Rubber: EDPM or NBR

Application range: Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight; radon tight

Features: tailor-made to meet requirements; segmented ring technology for adjustment to three or five different pipe diameters on site

Article Code: HRD SGi b40

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de