**ETGAR building developer package for building services outlets**

For buildings without a basement

For the distribution of power and communication lines from the building into the property. Comprising: Basic unit for setting in concrete with 4 outlets and a blind cover Height-adjustable installation fixture 30 m corrugated pipe DN 75 Locking sleeves for corrugated pipe Sealing caps for corrugated pipe Seal insert, gas- and water-tight Sleeve caps MS75K 2x13-21+3x7-13+1x5-12 with pipe section Sleeve caps MS75EW 1x24-40+3x7-13 with pipe section 1 piece of GMT lubricant

Application range: Water exposure class DIN 18533: W1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight

Features: Complete system for distributing the power supply to the entire property from the building connection room

Article Code: HAB ETGAR BHP

GTIN: -

Brand: Hauff-Technik

**Technical drawings**

[HAB ETGAR BHP Bemaßung (.PDF)](https://db.hauff-technik.de/files/840/3/BEMA_UNG_HAB_ETGAR_BHP_20240522_104951213.PDF)

Ctrl + click on the link to open in your browser

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de