**PE corrugated pipe**

For ETGAR BHP

Empty conduit system for extending the ETGAR building developer package for building services outlets.

Dimensions: OD: 75 mm

Material: PE

Tightness: gastight and watertight to 0.5 bar

Features: High degree of flexibility thanks to narrow radii

Article Code: HAB ETGAR WR75 GR30000

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de