**Standard internal corrugated pipe press seal**

Material: Press plates, screws and nuts: rust-free stainless steel V2A (AISI 304L); Rubber: EPDM

: Waterproof concrete stress class 1, waterproof concrete stress class 2

Tightness: gastight and watertight; radon tight

Features: segmented ring technology for adjustment to three or five different pipe diameters on site

Article Code: WIN SG b40 A2/EPDM

GTIN: -

Brand: Hauff-Technik

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de