**Standard press seal for internal sealing of corrugated pipes**

with segmented ring technology

Article Code: WIN SG b40 A2/EPDM

GTIN: -

Brand: Hauff-Technik

For sealing cables and communication lines inside of corrugated pipes. Split design for sealing new installed cables or cables that have already been installed. A corrugated pipe seal WRD or a comparable fastening must be installed to stabilize the corrugated pipe.

Dimensions: Sealing width: 40 mm; Press plates: 5 mm

Material: Press plates, screws and nuts: rust-free stainless steel V2A (AISI 304L); Rubber: EPDM

: Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight; radon-proof

Features: Segmented ring technology for adjustment on-site to pipe diameters

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de