**Single-line basic insert**

for buildings without a basement

Article Code: ESH Basic FUBO SR1 EBT

GTIN: -

Brand: Hauff-Technik

For the feeding in and sealing of supply lines (power, water, telecommunications or gas) through the base slab. Is supplemented with separately available spiral hose system, seal insert and utility sealing element.

Dimensions: Width: 222 mm; Length: 222 mm; Height: 270 mm

Material: Insert: ABS; Installation fixture: St37

Application range: Water exposure class DIN 18533: W1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight to 1.0 bar

Tests/Standards: DVGW VP 601

Features: variable height adaptation to the finished floor level; easy integration of the vapour barrier using the adhesive flange

**Technical drawings**

[Maße ESH Basic FUBO SR1 (.PDF)](https://db.hauff-technik.de/files/1008/3/BEMA_UNG_FUBO_SR1.PDF)

Ctrl + click on the link to open in your browser

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de