**Seal insert for basic insert**

Article Code: ESH Basic MBK SR1

GTIN: -

Brand: Hauff-Technik

Gastight and watertight building entry for gas, water, power or telecommunications services for buildings without a basement. The building entry is installed in the ESH Basic FUBO EBT SR1 basic unit. Gas valve/sealing element to seal the services are not included in the scope of supply (see accessories).

Dimensions: Width: 135 mm; Length: 135 mm; Height: 283 mm

Material: Anchor plate: glass fibre reinforced polyamide; Pipe: glass-fibre-reinforced polyamide with TPE; Screws: stainless steel V2A (AISI 304L)

Tightness: gastight and watertight to 1.0 bar

Tests/Standards: DVGW VP 601

Features: all-around smooth surface for optimum connection of the finished flooring

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de