**Universal wall sleeve**

for any type of wall

Article Code: UFR B

GTIN: -

Brand: Hauff-Technik

Easy installation in formwork, sealed on both sides ready for installation for flush setting in concrete. Can be cut to length on site to specific wall thickness using printed scale. Suitable for any type of wall. Tested according to FHRK test basis with FHRK quality seal.

Dimensions: Flange all-aroung: 50mm; Common wall thicknesses printed on the tube

Material: Pipe: PVC-U; Flange: ABS; 3-ribbed seals: EPDM; Closing cover: PE

Application range: Water exposure class DIN 18533: W1-E and W2.1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight

Features: printed scale for adjusting to specific wall thickness; Flange for plastic-modified bitumen thick coatings; Tested solution for use in pre-applied membrane sheet systems; Can be used in all wall types with three sealing levels

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de