**Floor drain with foil flange**

with backstop

Article Code: BALF RLS

GTIN: -

Brand: Hauff-Technik

Suitable for draining gray water in the floor area. Integrated backflow preventer prevents the waste water from flowing back. Gas- and watertight connection to the base plate with an integrated lip seal. Includes foil flange for connection to a bituminous thick coating, weldable membrane, or vapour barrier.

Dimensions: Top frame: 150 x 150 mm; Drain connection: DN 110; Foil flange: 500 x 500 mm

Material: Base body: PP; Drain grate: Stainless steel (AISI 304L); Lip seal: TPE; Foil flange: EPDM

Application range: Waterproof concrete stress class 1 and 2

Tightness: pressure-rated up to 5,0 bar; radon-proof

Features: frost-resistant backflow and odor barrier; Residue-free drainage of the water in the drain body; Prevention of clogging of the drain tank through dirt trap screen; Square foil flange

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de