**Wall penetration double socket**

Article Code: DMF

GTIN: -

Brand: Hauff-Technik

Wall penetration for connecting standard KG/HT pipes on both sides using push-in sleeves. Gas and watertight wall penetration thanks to integrated lip seal.

Material: KG socket: PVC-U / KG2000 socket: PP; KG2000 socket: PP; Lip seal: TPE

Application range: Waterproof concrete stress class 1 and 2

Tightness: pressure-rated up to 5,0 bar; radon-proof

Features: ready for wall installation; includes closing cover; pressure-resistant solid wall material

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de