**Single-line XL building package**

for buildings without a basement

Article Code: ESG100 FUBO BHPXL10m

GTIN: -

Brand: Hauff-Technik

XL building package in the form of a single-line building entry system suitable for gas, water or power supplies. Comprising: Basic insert for floor slab: ESG100 FUBO with factory-connected and tested empty conduit system Installation fixture, including water barrier flange Spiral hose 14110/10000 Sealing element: HRK100 SSG 1x18-65 b40 PAGF/A4/EPDM55Empty duct connection: ABEK95/102/110 1x18-65+2x16-20+2x12-16+2x5-10 b50

Dimensions: Basic insert ID: 100 mm; Spiral hose: Øi: 110 mm; Sealing element: area of application: 1 electric cable with Øa 18-65 mm, sealing width: 40mm; Sealing cap: for duct Øi: 95/102/110 mm, for lines Øa: 1x18-65, 2x5-10, 2x12-16, 2x16-20

Application range: Water exposure class DIN 18533: W1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight to 1.0 bar

Features: Tested pressure tight duct system; variable height adaptation to the finished floor level

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de