**Membrane injection system**

for buildings with a basement

Article Code: MIS60D E SET

GTIN: -

Brand: Hauff-Technik

For installation in all standard wall types to DIN 18533 and waterproof concrete to DIN 1045.

Dimensions: For core drills Ø: 62 - 65 mm; For wall thicknesses: from 200 to 1200 mm

Material: Flange, seal insert, counter-bearing and adapter: EPDM; Sealing tape: butyl; Resin injection hose: PE; Wall rosette: PE; Pipe: PVC-U; Wall terminator element: Flame-retardant polycarbonate

Application range: Water exposure class DIN 18533: W1-E and W2.1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight to 1.0 bar; radon-proof

Features: universal building entry with membrane injection system for core holes in the most common types of wall; Controlled resin discharge through slotted membrane hose; sealing lips ensure gentle seal for cables/pipes

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de