**Cement-coated wall sleeve**

with special coating

Article Code: ZVR

GTIN: -

Brand: Hauff-Technik

Easy installation in formwork, sealed on both sides ready for installation for flush setting in concrete. Special coating creates a tight bond with the building and balances out temperature variations. For lengths > 600 mm, the cement-coated wall sleeve is coated on each side by 250 mm. Tested according to FHRK test basis with FHRK quality seal.

Dimensions: Pipe length ≤ 600 mm: fully coated wall sleeve; Pipe length > 600 mm: partially coated wall sleeve

Material: Pipe: PVC-U; Closing cover: PE

Application range: Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight

Features: special coating creates a homogeneous bond with the concrete; Full surface sealing of the wall sleeve due to special coating; includes closing cover

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de