**Renovation wall sleeve**

Article Code: SFR

GTIN: -

Brand: Hauff-Technik

For retrofit installation in bricks or concrete walls.

Dimensions: Wall thickness: 4, 5 and 6 mm

Material: Pipe: PVC-U

Application range: Waterproof concrete stress class 1 and 2

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de