**Outer sealing element module 4**

for single-line building entry systems basic variant 1

Article Code: FLFA 100 DIN18533

GTIN: -

Brand: Hauff-Technik

Outer sealing element for ESH Basic - BV 1 with fixed/loose flange for buildings with a basement with waterproof sheeting for standing/pressing water load case to DIN 18533, W2.2-E. Suitable for holding bitumen or foil waterproof sheeting.

Dimensions: Fixed flange OD: 420 mm; Loose flange OD: 410 mm; Thickness of fixed flange: 10 mm; Thickness of loose flange: 10 mm

Material: Stainless steel V2A (AISI 304L)

Application range: Water exposure class DIN 18533: W1-E, W2.1-E and W2.2-E

Tightness: gastight and watertight to 1.0 bar

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de