**Insulated earthing entry**

Article Code: HEA IS

GTIN: -

Brand: Hauff-Technik

Isolated earthing entry for installation flush with the formwork during formwork work, for an earthing connection that is electrically isolated from the building, tested short-circuit current load, M12 watertight connection thread on both sides.

Dimensions: Conductor core: round, Ø 25 mm; Contact washer: Ø 72 mm; Minimum wall thickness: 70 mm

Material: Conductor core and contact washers: stainless steel V4A (AISI 316L); Protective cover: cellular rubber; Electrical insulation: EPDM; Water barrier: EPDM

Application range: Waterproof concrete stress class 1 and 2

Tests/Standards: according VDE 0101, EN 50522

Features: Patented anti-twist protection thanks to the special shape of the contact disc

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de