**Earthing entry**

for retrofit installation

Article Code: HEA N

GTIN: -

Brand: Hauff-Technik

Earthing entry, seal with the wall is made on both sides with a flat gasket which is pressed against the wall with nuts. A terminal lug with cross-clamp is used to connect flat and/or round steels.

Dimensions: Contact washer: Ø 72 mm; Conductor core: M16 threaded rod; Required drill hole: 20 mm; Wall thicknesses: up to 600, thicker walls on request

Material: All metal parts: stainless steel V4A (AISI 316L); Seal: EPDM

Application range: Waterproof concrete stress class 1 and 2

Tests/Standards: DIN 18014; DIN EN 62305-3; VDE 0185-305-3 (with lightning protection application)

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de