**Earthing entry**

for building entry according to DIN 18533 (black tank)

Article Code: HEA W

GTIN: -

Brand: Hauff-Technik

Earthing entry, manufactured to DIN 1853, watertight connection thread on both sides.

Dimensions: Fixed/loose flange: OD 210 mm; Conductor core: round, Ø 25 mm; Conductor core connection: with M16 threaded bolt; Contact washer: Ø 72 mm; Minimum wall thickness: 180 mm

Material: Fixed/loose flange: V4A (AISI 316L); Conductor core and contact washers: stainless steel V4A (AISI 316L); Conductor core connection: St37 galvanised; Protective covers: PE; M20 cross-clamp: stainless steel V4A (AISI 316L)

Application range: Water exposure class DIN 18533: W1-E, W2.1-E and W2.2-E

Tests/Standards: To DIN 18014; DIN EN 62305-3; VDE 0185-305-3 (with lightning protection application)

Features: Patented anti-twist protection thanks to the special shape of the contact disc

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de