**Earthing entry**

for double walls/element walls

Article Code: HEA EW

GTIN: -

Brand: Hauff-Technik

Earthing entry, for installation in prefabricated construction, M12 watertight connection thread on both sides.

Dimensions: Conductor core: round, Ø 25 mm; Conductor core connection: with M16 threaded bolt; Contact washer: Ø 72 mm; Minimum wall thickness: 170 mm

Material: Conductor core and contact washers: stainless steel V4A (AISI 316L); Conductor core connection: St37 galvanised; Water barriers: NBR, EPDM; Protective covers: PE

Application range: Waterproof concrete stress class 1 and 2

Tests/Standards: DIN 18014; DIN EN 62305-3; VDE 0185-305-3 (with lightning protection application)

Features: three water barriers; Patented anti-twist protection thanks to the special shape of the contact disc

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de