**Flexible earthing entry**

Article Code: HEA PF

GTIN: -

Brand: Hauff-Technik

Earthing entry with flexible steel cable for positioning earthing connections which can be adjusted both up and down and from side to side. Reinforcement connection can be created with cross-clamp if required, watertight connection thread on both sides, set in concrete in several sections.

Dimensions: Conductor core: round, Ø 25 mm; Contact washer: Ø 72 mm; Steel cable: Ø 10 mm

Material: Conductor core and contact washers: stainless steel V4A (AISI 316L); Steel cable: galvanised; Water barrier: NBR; Protective covers: PE

Application range: Waterproof concrete stress class 1 and 2

Tests/Standards: DIN 18014; DIN EN 62305-3; VDE 0185-305-3 (with lightning protection application)

Features: Patented anti-twist protection thanks to the special shape of the contact disc

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de