**Cross-clamp**

Article Code: HEA KKL

GTIN: -

Brand: Hauff-Technik

Cross-clamp for screwing into the connection thread of earthing entries and earthing fixed points, can be used to connect round or flat steel.

Dimensions: Length: approx. 50 mm; For flat earthing strap 40 x 5 or round earthing conductor Rd 8 - 12

Material: St37 galvanised or stainless steel V4A (AISI 316L)

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de