**Standard press seal**

with stepped variable super segmented ring technology

Article Code: HSD SSG

GTIN: -

Brand: Hauff-Technik

Split press seal for sealing new media pipes/ducts to be installed or media pipes/ducts that have already been laid in core drills or wall sleeves. Tested according to FHRK test basis with FHRK quality seal.

Dimensions: Sealing width: 40 mm

Material: Press plates, screws and nuts: rust-free stainless steel V2A (AISI 304L) or V4A (AISI 316L); Rubber: EPDM

Application range: Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight; radon-proof

Features: Visual and physical installation control thanks to integrated inspection opening; integrated super segmented ring technology for individual adjustment to cable/pipe diameter on site; Segments with diameter marking

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de