**Membrane injection system**

for buildings without a basement

Article Code: MIS90S

GTIN: -

Brand: Hauff-Technik

For sloping entry through the wall or floor slab in all common types of wall to DIN 18533 and waterproof concrete to DIN 1045.

Dimensions: For core drills ID: 92 - 102 mm; Overall length: 1300 mm

Material: Flange, counter-bearing, sleeve cap, membrane hose: EPDM; Resin filler hose: PE; Pipe: PVC-U; End cap: ZK/NBR (butadiene/acrylonitrile rubber); Stainless steel clamping straps: V2A (AISI 304L)

Application range: Water exposure class DIN 18533: W1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight to 1.0 bar

Features: universal building entry with membrane injection system for sloping drill holes through floor slabs or walls; simultaneous sealing of power, water and communication services; controlled ejection of resin through slit membrane hose

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de