**Basic insert**

for buildings without a basement

Article Code: ESG150 FUBO EBTMA

GTIN: -

Brand: Hauff-Technik

Basic insert and installation fixture for setting in concrete in the floor slabs of buildings without a basement. For the compact entry of gas or water services, DN 80. The combined building entry HEK and the flexible spiral hose are not included in the scope of delivery.

Dimensions: Basic insert: ID 150 mm

Material: Basic insert: PVC-U; Sleeve: EPDM; Water barrier flange: EPDM; Installation fixture: St37

Application range: Water exposure class DIN 18533: W1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight to 1.0 bar

Features: variable height adaptation to the finished floor level

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de