**Earthing entry**

for retrofit installation

Article Code: HEA ND

GTIN: -

Brand: Hauff-Technik

Earthing entry for existing walls with perimeter insulation. Sealing to the wall is provided on both sides by a surface seal, which is pressed to the wall with nuts. Flat or round earthing straps can be connected using a connection lug with cross clamp.

Dimensions: Contact washer: Ø 72 mm; Conductor core: M16 threaded rod; Required drill hole: 20 mm; For wall thicknesses up to 400 mm, thicker walls on request; For perimeter insulation: up to 200 mm

Material: All metal parts: stainless steel V4A (AISI 316L); Seal: EPDM

Application range: Waterproof concrete stress class 1 and 2

Tests/Standards: DIN 18014; DIN EN 62305-3; VDE 0185-305-3 (with lightning protection application)

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de