**Basic variant with inner seal for district heating**

for buildings with a basement

Article Code: MSH FW Basic GV2

GTIN: -

Brand: Hauff-Technik

For the collective feeding in and sealing of all supply lines (district heating, water, power and telecommunications). The multi-line building entry system MSH-FW Basic – basic variant 2 is a basic module. It is supplemented by the following closed sealing elements and modules which are available to purchase separately: MSH sealing elements set (closed sealing elements) MSH-FW module 6: outer sealing element with sealing width 90 mm (for installation in double walls/element walls) MSH-FW module 6 and module 2: outer sealing element with sealing width 90 mm and external flange for the integration of existing building seals Additional supplements are possible.

Dimensions: Inner seal with 60 mm sealing width; Compatible with core drill/wall sleeve: ID: 298 mm - 303 mm; Maximum wall thickness: 500 mm (special lengths on request)

Material: Inner seal: die-cast aluminium/EPDM; Sleeve pipes: PVC; Screws and washers: stainless steel V2A (AISI 304L)

Application range: Water exposure class DIN 18533: W1-E and W2.1-E; Waterproof concrete stress class 1 and 2

Tightness: gastight and watertight to 1.0 bar

Features: Visual and physical installation control thanks to integrated inspection opening; integrated leak test equipment for double walls/element walls for certainty during installation

**Hauff-Technik GmbH & Co. KG**

**Manufacturer information**

Hauff-Technik GmbH & Co. KG
Robert-Bosch-Straße 9
89568 Hermaringen, GERMANY

Telefon +49 73 22 13 33 - 0
Fax +49 73 22 13 33 - 999
office@hauff-technik.de
http://www.hauff-technik.de